|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Date:** |  | **New** | **** | **Revised** |  | **Page** |  |

**TRADE:** **POLYSTYRENE PANEL CLADDING INSTALLER**

|  |  |  |  |
| --- | --- | --- | --- |
| **Client:** | **Irvine & Brooks** | **Job No:** | **7869/17** |
| **Address:** | **72 Middle Street, Kingsford.** | **Supervisor:** |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Key:** | “1” action now | “2” action ASAP | “3” action ASAP |

**Note 1:** Refer to the general Safety Plan and your Safe Work Method Statement prepared in accordance with WHS Regulation 2017 s309-315 Part 6.4

**Note 2:** Safe work procedures shall be implemented for the supply and use of a *hazardous chemical / substance/s* on site that complies with the *current material safety data sheet* recommendations and also complies with the requirements of WHS Regulation 2017 Chapter 3 - Part 3.2

**Note 3:** All *manual tasks* are to comply with the requirements of WHS Regulation 2017 - Hazardous manual tasks Part 4.2 or Safe Work Australia - National Code of Practice for Manual Handling 2009 [or as amended] or Safe Work NSW Code of Practice - Hazardous manual tasks

**Note 4:** Management of the risk of fall from one level to another must comply with Part 3.1 and the requirements of WHS Regulation 2017 - Falls s78-80 Part 4.4

**Note 5:** **Review of Control Measures - *If there are any tasks that may be included by way of variation to the plans or an alternative approach to the set task,*** ***it is a requirement to carry out a “specific Risk Assessment” for the task or tasks.***

| Job Step / Hazard | Potential Harm | Likelihood | | | Result | | | **Priority** | Possible Controls | Responsible Person/s | Date |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Likely** | **Possible** | **Unlikely** | **Major** | **Severe** | **Minor** |
| Access to site / work areas -  Slips, trips, falls and accessibility -  Access ways not clearly defined | Slips, trips and falls |  |  |  |  |  |  | 3 | Identify the risks and plan the tasks in consultation with the *‘workers’*  Assess travel path and distance to work area  All “*workers*” to register attendance via Cape Cod QR scanner before entering the site; to read the General Construction Safety Plan signage; and to read the Site Specific Risk Assessment.  Ensure unobstructed all weather access to site and work areas.  Unload and move equipment and materials to designated area to keep footpath / work place access clear | Site Supervisor / all ‘*workers’* |  |
| Stored materials -  Slips, trips, falls and accessibility -  Access ways not clearly defined | Slips, trips and falls |  |  |  |  |  |  | 2 | Assess travel path and distance to work area  Ensure unobstructed access to work areas.  Provide and maintain barricades to isolate material and to restrict access.  Provide designated waste areas | Site Supervisor / all ‘*workers’* |  |
| Manual tasks | Muscle strain -back injuries and cuts  Over exertion or repetitive movements |  |  |  |  |  |  | 2 | Identify the risks and plan the tasks in consultation with the *‘workers’*  Use task specific trained ‘*workers’* and team lifting.  Rotate *‘workers’* and vary tasks. | Contractor / all ‘*workers’* |  |
| Exposure to noise  Plant / equipment | Hearing damage |  |  |  |  |  |  | 2 | Isolate plant and equipment.  Use appropriate PPE | Contractor / all ‘*workers’* |  |
| Exposure to UV light / weather -  UV light - glare  Extreme temperatures | Skin cancer / sun burn -  Dehydration - heat stroke or fatigue  Sight damage |  |  |  |  |  |  | 2 | Reduce exposure where possible.  Monitor *‘workers’* condition  Adequate fluid intake  Use appropriate sun screen.  Wear appropriate PPE. | Contractor / all ‘*workers’* |  |
| Exposure to polystyrene dust- | Dust inhalation - respiratory problems  Eye and skin irritations / allergies |  | 🗸 |  |  |  |  | 2 | Appropriate procedures to contain dust.  Monitor for airborne dust/ fibres when handling or cutting panels  Use appropriate PPE - disposable dust protection.  Provide Safety Data Sheet. | Contractor / all ‘*workers’* |  |
| Contact with o/head electrical services / point of attachment -  Power lines not isolated, covered or enclosed -  Working to close to electrical supply -Strong winds causing power lines to swing close to work area -  Wet conditions making ‘tiger tails’ ineffective | Electric shock or electrocution |  |  |  |  |  |  | 3 | Identify that the electrical service is isolated prior to work commencing.  Provide ‘tiger tails’ [insulation] - adequately boxed adjacent to scaffold - extended an appropriate distance past the boundary | Licensed Electrical Contractor or Approved person  Site Supervisor  Contractor / all ‘*workers’* |  |
| Working at height from scaffold / work platform / roof surface -  Slips, trips, falls and accessibility -  Inadequate fall arrest system /work platform -  Windy and or wet conditions -  Pitch of roof and roofing material -  Gravity - overbalancing | Slips, trips and falls from scaffold or work platform  Fractures, bruises lacerations and personal injuries |  |  |  |  |  |  | 3 | Identify the risks and plan the tasks in consultation with the *‘workers’*  Assess travel path and distance to work area  Ensure unobstructed access to work areas.  Scaffold guardrails and work platform is complete - work platform clean and dry.  Perimeter and edge protection when working from roof surface  Train ‘*workers’* in safe working at heights.  Limit the use of ladders | Contractor / all ‘*workers’* |  |
| Carry cladding panels, materials and tools up ramp  / scaffold - installation of the cladding panels -  Slips, trips, falls and accessibility -  Inadequate fall protection system / work platform -  Slope of ramp -  Windy and or wet conditions -  Manual tasks  Exposure to dust -  Hazardous chemicals -  Biological | Slips, trips and falls from ramp or work platform  Muscle strain -back injuries and cuts  Dust inhalation - respiratory problems  Eye and skin irritations / allergies |  |  |  |  |  |  | 3 | Identify the risks and plan the tasks in consultation with the *‘workers’*  Assess travel path and distance to work area  Ensure unobstructed access to work areas  Guardrails to ramp are in place - ramp and work platform clean and dry.  Scaffold guardrails and work platform is complete - use of toe boards /dust screening.  Provide and maintain appropriate warning signage and barricades to isolate and to restrict unauthorised / inadvertent access / entry around / under the work area by *others*  Use task specific trained *‘workers’* - team lifting and carrying - windy conditions  Rotate *‘workers’* and vary tasks  Limit weights to manageable sizes.  Appropriate procedures to contain dust resulting from cutting of the panels  Ensure panels and waste are secured on windy days  Use appropriate PPE - disposable dust / fibre protection.  Don’t use step ladder to gain extra height from scaffold work platform.  SWMS | Contractor / all ‘*workers’* |  |
| Use of electrical powered / battery operated tools -  Electricity -  Exposure to noise -  Exposure to dust -  Hazardous chemicals -  Biological -  Plant / equipment - | Electric shock or electrocution  Hearing loss  Inhalation of dust - respiratory problems.  Eye and skin irritations / allergies -  Sight damage |  |  |  |  |  |  | 2 | Identify the risks and plan the task in consultation with the *‘workers’*  Protect power lead from damage - power saw blade / sharp edges / vehicular traffic  Use stands and hooks for leads in trafficable areas  Guards to power tools fully operational.  Monitor for airborne dust/ fibres  Adequate ventilation and lighting  Use of appropriate PPE.  Use task specific trained ‘*workers’*. | Contractor / all ‘*workers’* |  |
| Site clean up on completion of work  Manual tasks  Exposure to dust -  Hazardous chemicals  Biological - | Inhalation of dust - respiratory problems.  Eye and skin irritations / allergies  Personal injuries - cuts and abrasions.  . |  |  |  |  |  |  | 3 | Place all waste polystyrene material in heavy duty plastic sheeting and seal.  Place general waste in designated waste area / skip bin  Leave site / work area including scaffold working platform in a clean and tidy condition  Remove any temporary barricades if no longer required | Contractor / all ‘*workers’* |  |

I / We have consulted with Cape Cod Australia Pty. Limited and have mutually agreed on the above procedures. This risk assessment provides details on how I / We will manage my / our work on this Cape Cod Australia Pty. Limited work site.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Company Name: |  |  | Signed by: |  |
|  |  |  | for and on behalf of: | Cape Cod Australia Pty. Ltd |
| Signed by: |  |  |  | ABN: 54 000 605 407 |
|  | (Contractor PCBU) |  |  | Builder’s Licence No. 5519 |
| ABN: |  |  |  |  |
| Address: |  |  |  |  |
|  |  |  |  |  |
| Phone: |  |  |  |  |
| Email: |  |  |  |  |