|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Date:** |  | **New** | **** | **Revised** |  | **Page** |  |

**TRADE:** **TEXTURE COATING APPLICATOR**

|  |  |  |  |
| --- | --- | --- | --- |
| **Client:** | **Tamas** | **Job No:** | **7845/17** |
| **Address:** | **1 Mocatta Avenue, Pymble** | **Supervisor:** |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Key:** | “1” action now | “2” action ASAP | “3” action ASAP |

**Note 1:** Refer to the general Safety Plan and your Safe Work Method Statement prepared in accordance with WHS Regulation 2017 s309-315 Part 6.4

**Note 2:** Safe work procedures shall be implemented for the supply and use of a *hazardous chemical / substance/s* on site that complies with the *current material safety data sheet* recommendations and also complies with the requirements of WHS Regulation 2017 Chapter 3 - Part 3.2

**Note 3:** All *manual tasks* are to comply with the requirements of WHS Regulation 2017 - Hazardous manual tasks Part 4.2 or Safe Work Australia - National Code of Practice for Manual Handling 2009 [or as amended] or Safe Work NSW Code of Practice - Hazardous manual tasks

**Note 4:** Management of the risk of fall from one level to another must comply with Part 3.1 and the requirements of WHS Regulation 2017 - Falls s78-80 Part 4.4

**Note 5:** **Review of Control Measures - *If there are any tasks that may be included by way of variation to the plans or an alternative approach to the set task,*** ***it is a requirement to carry out a “specific Risk Assessment” for the task or tasks.***

| Job Step / Hazard | Potential Harm | Likelihood | | | Result | | | **Priority** | Possible Controls | Responsible Person/s | Date |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Likely** | **Possible** | **Unlikely** | **Major** | **Severe** | **Minor** |
| Access to site / work areas -  Slips, trips, falls and accessibility -  Access ways not clearly defined | Slips, trips and falls |  |  |  |  |  |  | 3 | Identify the risks and plan the tasks in consultation with the *‘workers’*  Assess travel path and distance to work area  All “*workers*” to register attendance via Cape Cod QR scanner before entering the site; to read the General Construction Safety Plan signage; and to read the Site Specific Risk Assessment.  Ensure unobstructed all weather access to site and work areas.  Unload and move equipment and materials to designated area to keep footpath / work place access clear | Site Supervisor / all ‘*workers’* |  |
| Stored materials -  Slips, trips, falls and accessibility -  Access ways not clearly defined | Slips, trips and falls |  |  |  |  |  |  | 2 | Assess travel path and distance to work area  Ensure unobstructed access to work area.  Provide and maintain barricades to isolate material and to restrict access.  Provide designated waste areas | Site Supervisor / all ‘*workers’* |  |
| Manual tasks | Muscle strain - back injuries  Over exertion or repetitive movements |  |  |  |  |  |  | 2 | Identify the risks and plan the tasks in consultation with the *‘workers’*  Use task specific trained ‘*workers’* - rotate *‘workers’* and vary tasks. | Contractor / all ‘*workers’* |  |
| Exposure to UV light / weather -  UV light - glare  Extreme temperatures | Skin cancer / sun burn -  Dehydration - heat stroke or fatigue  Sight damage |  |  |  |  |  |  | 2 | Reduce exposure where possible.  Monitor *‘workers’* condition  Adequate fluid intake  Use appropriate sun screen.  Wear appropriate PPE. | Contractor / all ‘*workers’* |  |
| Exposure to dust/ chemical vapours -  Hazardous chemical - Biological - | Dust and chemical vapour inhalation / skin and eye allergies/ irritations.  Respiratory problems |  |  |  |  |  |  | 2 | Use appropriate PPE - disposable dust / chemical vapour protection. | Contractor / all ‘*workers’* |  |
| Use of battery operated / electrical  powered plant  and equipment -  Electricity -  Exposure to noise - | Electrical shock or electrocution  Hearing loss  Sight damage |  |  |  |  |  |  | 2 | RCD installed on mains supply / portable generator  Protect power lead from damage  sharp edges / vehicular traffic  Use stands and hooks for leads in trafficable areas  Guards to plant and equipment fully operational.  Use of appropriate PPE.  Use task specific trained ‘*workers’* | Contractor/ all *‘workers’* |  |
| Carry mixed  texture coating to work area using bucket -  Slips, trips, falls and accessibility -  Manual tasks | Slips, trips and falls.  Back injury - muscle strain / sprain - cuts |  |  |  |  |  |  | 2 | Identify the risks and plan the task in consultation with the *‘workers’*  Assess travel path and distance to work area  Ensure unobstructed access to work areas.  Use task specific trained ‘*workers’* and rotate *‘workers’ tasks*.  Limit the weight of each bucket load to easily manageable size.  SWMS | Contractor / all ‘*workers’* |  |
| Carry mixed  texture coating, tools to ground floor work area -  Slips, trips, falls and accessibility -  Inadequate work platform -  Site and weather conditions -  Gravity - overbalancing  Manual tasks | Slips, trips and falls from scaffold / work platform or step ladder  Muscle strain -back injuries and cuts  Over exertion or repetitive movements*.* |  |  |  |  |  |  |  | Identify the risks and plan the tasks in consultation with the *‘workers’*  Assess travel path and distance to work area  Ensure unobstructed access to work areas.  Use task specific trained and experienced *‘workers’ -* rotate *‘workers’* and vary tasks.  Scaffold located on level ground or firm secure surface.  Guardrails to scaffold are in place - work platform is complete  Use approved step ladder  Limit the use of step ladders | Contractor/ all *‘workers’* |  |
| Carry mixed  texture coating and tools up ramp  / scaffold -  Slips, trips, falls and accessibility -  Slope of ramp -  Weather conditions - wet  Manual tasks | Slips, trips and falls from ramp / scaffold.  Back injuries - muscle sprains, strains and cuts |  |  |  |  |  |  | 2 | Identify the risks and plan the task in consultation with the *‘workers’*  Assess travel path and distance to work area  Ensure unobstructed access to work areas.  Guardrails to ramp are in place - ramp and work platform clean and dry.  Scaffold guardrails and work platform complete - use of toe boards /dust screening.  Use task specific trained *’workers’* - rotate *‘workers’* and vary tasks. | Contractor / all ‘*workers’* |  |
| Working at height from scaffold / work platform / roof surface -  Slips, trips, falls and accessibility -  Inadequate fall arrest system /work platform -  Windy and or wet conditions -  Pitch of roof and roofing material -  Gravity - overbalancing | Slips, trips and falls from scaffold or work platform / roof surface  Fractures, bruises lacerations and personal injuries |  |  |  |  |  |  | 3 | Identify the risks and plan the tasks in consultation with the *‘workers’*  Assess travel path and distance to work area  Ensure unobstructed access to work area  Provide and maintain appropriate warning signage and barricades to isolate and to restrict unauthorised / inadvertent access / entry around / under the work area by *others*  Scaffold deck complete - use of toe boards / dust screening  Perimeter and edge protection when working from roof surface  Maintain clean work area  Train ‘*workers’* in safe working at heights.  Don’t use step ladder to gain extra height from scaffold work platform.  Limit the use of ladders | Contractor / all ‘*workers’* |  |
| Application of the texture coating -  Manual tasks -  Hazardous chemicals -  Biological - | Muscle strain - back injuries and cuts  Over exertion or repetitive movements  Inhalation of fumes -respiratory problems.  Eye and skin irritations/ allergies |  |  |  |  |  |  | 3 | Identify the risks and plan the tasks in consultation with the *‘workers’*  Use task specific trained and experienced ‘*workers’* - rotate *‘workers’* and vary tasks.  Ensure adequate ventilation.  Use of appropriate PPE and provide SDS. | Contractor / all ‘*workers’* |  |
| Use of gap filling flexible fillers / sealants -  Hazardous chemicals -  Biological | Inhalation of fumes - respiratory problems.  Eye and skin irritations/ allergies |  |  |  |  |  | 3 |  | Identify the risks / hazards and plan the task in consultation with the *‘workers’*  Avoid contact with skin and eyes.  Monitor air quality for chemical vapours  Use task specific trained ‘*workers*’.  Use appropriate PPE. Provide SDS. | Contractor / all ‘*workers’* |  |
| Step ladder  access  to work area -  Slips, trips, falls and accessibility -  Gravity - overbalancing | Fall from ladder |  |  |  |  |  |  | 1 | Identify the risks and plan the task in consultation with the *‘workers’*  Use task specific trained ‘*workers’.*  Don’t use step ladder to gain extra height from scaffold work platform.  Use approved ladder.  Limit the use of ladders. | Step ladder  access  to work area -  Slips, trips, falls and accessibility -  Gravity - overbalancing |  |
| Work from extension ladder  Slips, trips, falls and accessibility -  Gravity - overbalancing | Fall from ladder |  |  |  |  |  |  | 3 | Identify the risks and plan the task in consultation with the *‘workers’*  Use scaffold as working platform.  Ensure ladders are at 4:1 slope.  Secure ladder at base and top.  Ensure ‘*workers’* face the ladder when climbing up and down ladder.  Provide and maintain appropriate warning signage and barricades to isolate and to restrict unauthorised / inadvertent access / entry into the work area by *others*.  Limit the use of ladders | Contractor / all ‘*workers’* |  |
| Finishing to window sills and reveals, corbels, architraves and gables -  Slips, trips, falls and accessibility -  Inadequate fall arrest system /work platform -  Windy and or wet conditions -  Gravity - overbalancing  Manual tasks | Slips, trips and falls from scaffold / work platform / roof surface  Fall from ladder  Muscle sprains /strains |  |  |  |  |  |  | 2 | Identify the risks and plan the tasks in consultation with the *‘workers’*  Use scaffold as working platform.  Perimeter and edge protection when working from roof surface.  Use task specific trained ‘*workers’*.  Ensure ladders are at 4:1 slope.  Secure ladder at base and top.  Ensure ‘*workers’* face the ladder when climbing up and down.  Limit the use of ladders | Contractor / all ‘*workers’* |  |
| Oil based coating and solvents - mixing and clean up -  Hazardous  chemicals -  Biological | Inhalation of fumes - respiratory problems.  Eye and skin irritations/ allergies |  |  |  |  |  |  | 3 | Identify the risks and plan the task in consultation with the *‘workers’*  Substitute material with safer low to no volatile organic compounds [VOC] and avoid contact with skin and eyes.  Use task specific trained ‘*workers*’.  Use appropriate PPE. Provide SDS. | Contractor / all ‘*workers’* |  |
| Site clean up on completion of work  Manual tasks  Exposure to dust -  Hazardous chemicals  Biological - | Inhalation of dust - respiratory problems.  Eye and skin irritations / allergies  Personal injuries - cuts and abrasions. |  |  |  |  |  |  | 3 | Place all associated waste and rubbish in the designated waste area / skip bin  Leave site / work area including scaffold work platform in a clean and tidy condition  Remove any temporary barricades if no longer required | Contractor / all ‘*workers’* |  |

I / We have consulted with Cape Cod Australia Pty. Limited and have mutually agreed on the above procedures. This risk assessment provides details on how I / we will manage my / our work on this Cape Cod Australia Pty. Limited work site.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Company Name: |  |  | Signed by: |  |
|  |  |  | for and on behalf of: | Cape Cod Australia Pty. Limited |
| Signed by: |  |  |  | ABN: 54 000 605 407 |
|  | (Contractor PCBU) |  |  | Builder’s Licence No. 5519 |
| ABN: |  |  |  |  |
| Address: |  |  |  |  |
|  |  |  |  |  |
| Phone: |  |  |  |  |
| Email: |  |  |  |  |